Title: 
Installing Hardwood Flooring – Tips To Make Your Job Go Smoother

Word Count:
455

Summary:
It’s not so hard installing laminate flooring, but you need to know how. There are clear directions


Keywords:
installing hardwood flooring, directions for installing laminate flooring, install glueless laminate flooring


Article Body:
Installing hardwood flooring can take place in several ways depending on the type of hardwood flooring that you have. If you have solid hardwood, you have to look at the type of wood you have. You can have parquet flooring, which usually comes in tiles of 6 inches by 6 inches or strips or planks that can be as much as 3 inches wide. If you have laminate wood flooring then you have to look at a different method of installing hardwood flooring.

Whether you choose laminate flooring or solid hardwood flooring, the directions for installing both of them are printed on the inside of the packaging. If you have previously installed hardwood floors and now you want to install glueless laminate flooring, you do need to read the directions for installing laminate flooring. When you are installing hardwood flooring made of solid wood, you have to open the packages and let the wood become acclimatized to the humidity and temperature of your home. With laminate flooring, you have to do the exact opposite. You should not take this flooring out of the package until you are ready to start installing. 

Successful installation of hardwood or laminate flooring depends upon careful planning. Even if you are installing hardwood flooring over an existing concrete or vinyl floor, you do have to sweep and vacuum the floor to remove all the dust and dirt. If you are not sure of exactly how much laminate flooring you will need, the directions for installing laminate flooring also include directions for measuring the room to calculate the amount of flooring that you need. When you intend to install glueless laminate flooring, you can also bring your measurements into your local flooring store and have the experts do the calculations for you. 

If you are wondering how to install glueless laminate flooring and be able to keep it on the floor, each of the planks lock together with the tongue and groove design. When installing hardwood flooring like this, you cannot glue, nail or staple it in any way. When you start installing always consider the way the light shines into the room. Begin laying the planks toward the light and in a hallway always install glueless laminate flooring lengthwise. 

The directions for installing laminate flooring will tell you that you lay the first plank with the grooves against the wall. Place spacers where they are needed when installing hardwood flooring between the wall and the plank to maintain ½ inch extension gap. You will have to mark and cut the planks as you are installing the flooring because they are of random lengths. Always begin in a corner when installing hardwood flooring and the first board in the row should be a full plank.


