Title: 
Driveway Cracking? How To Concrete Resurface Quickly and Easily

Word Count:
365

Summary:
Concrete resurfacing is a method of repairing concrete sections when they are cracking or discolored.  This usually happens over time and concrete resurfacing will help restore the look of the area to one that is much more attractive.


Keywords:
concrete resurfacing,concrete repair,concrete crack repair,concrete sealing,epoxy mortar,sealer, concrete


Article Body:
Concrete resurfacing is a method of repairing concrete sections when they are cracking or discolored.  This usually happens over time and concrete resurfacing will help restore the look of the area to one that is much more attractive.  There is also decorative concrete resurfacing which still restores the look of the concrete but also adds a decorative touch to it.  This can include color and designs that can get very elaborate.  Some refinishing projects are like works of art and are very beautiful.  Prices for concrete resurfacing vary depending on the type of project you want and how elaborate you want to get in your designs.  Typically, though, it starts off at approximately three dollars per square foot and can increase to over seven dollars per square foot.  

The first thing that is done in concrete resurfacing is the cleaning of the area.  This is usually done with a pressure washer to ensure all built up dirt and debris is removed.  Next, there are several steps in repairing the cracks that may be found in the concrete.  Cracks are first primed then filled with crack repair material.  Then, they are reinforced with fabric and then a base coat is painted over the fabric.  Polymer concrete is then smoothed on to the surface over the crack and ground down once dry until it is smooth and even.  After the cracks are repaired, any holes that are in the concrete will be filled with epoxy mortar.  Now that the concrete is thoroughly repaired, it is time to start the concrete resurfacing.

The prime coat and granule broadcast will be applied now that all the cracks and holes are repaired.  A texture coat will be added next.  First you will need to mix it according to package specifications.  Then the mixture will be sprayed over the area using a special type of spray gun.  Once complete, the surface should be run over with a trowel to ensure an even surface.  You should work from the top and go backwards down the area for this.  The color coat is next, adding the particular color you want for your area.  Then a sealer is used to finish off the project.


