Title: 
Preventing Bathroom Mold

Word Count:
417

Summary:
As the most frequently wetted area in your home, the bathroom is where mold is most likely to grow. However, with some attention and proper maintenance, it is easy to prevent mold from growing and spreading in your bathroom.


Keywords:



Article Body:
Your bathroom is one of the most wetted rooms in your home, and therefore is one of the rooms where mold is most likely to grow. The fact that heat and moisture are frequently generated in the bathroom promotes mold growth as these factors provide great conditions for mold to grow and flourish. Prevent mold in your bathroom is vital for your health and for the way your bathroom looks. In addition, if neglected and due to optimal growing conditions, bathroom mold is likely to spread internally through walls, ceilings, and floors, leading to an extremely expensive remediation costs. One of the key factors for bathroom mold prevention is frequent inspections to prevent water damage that can lead to mold growth. The first step in mold prevention is keeping your bathroom dry and airy. Use a humidity meter to check humidity levels before and after showers. Be sure to keep humidity levels below forty to forty five percent. If you allow adequate air circulation, your bathroom humidity levels should drop below 45 percent within 5-10 minutes from the minute you finished your shower.

Shower and Bathtub Maintenance

Keep the bathtub, floors, walls, and ceilings, clean and dry at all times. To prevent mold where it is very likely to grow, be sure to stretch the bathtub curtain after using the bathtub to allow equal and complete drying. 

Air Flow

Allowing air flow and air circulation are key step in keeping low humidity levels. The basic technique and the simplest is to open windows and doors right after taking a shower to allow air to free flow and remove excess moisture. If you didn’t install an exhaust fan yet, do so as soon as possible as this is a great tool for bathroom ventilation. Turn on the exhaust fan while taking a bath or shower and leave it working for 5-10 more minutes after finishing using the bathroom to allow the bathroom to dry completely. Confirm that your fan exhausts outdoors directly.

Day to Day Maintenance 

Day to day maintenance is important to prevent water damage and mold. It will also help detecting problems before they become a large scale disaster. Drains must be kept in good shape. Allow the bathtub to drain completely and by removing all debris and using drain openers from time to time. Create hard surfaces on your bathroom walls using semi-gloss paint. It is harder for mold to grow on these type of surfaces. 

For more information visit http://restorationsos.com 
Free guides are available


