Title: 
Installing Laminate Flooring – Tips To Make Installation Easier

Word Count:
539

Summary:
Installing laminate flooring isn’t so  hard, as long as you know what to do.


Keywords:
installing laminate flooring, how to install laminate flooring, installing hardwood flooring


Article Body:
Installing laminate flooring is something that you can easily do yourself. Why pay professionals to do it when the instructions for how to install it are printed right on the package. In addition, all the manufacturers of laminate flooring have the directions for installing the flooring available on their websites. There are some differences in how to install laminate floors and installing hardwood floors, but you can use the same tools for both. The first step in installing laminate flooring is to calculate the size of the room and purchase the flooring of your choice. 

When installing hardwood flooring, you have to leave the hardwood open for a time so that it can become acclimatized to your home. This is not the case when installing laminate flooring. When reading the directions as to how to install laminate flooring, you will learn that you have to install it as soon as you open the package. You also have to check all the planks before you install them to ensure that none of them are defective. You will get a refund for any defective planks, but not if you have already installed them. If you have difficulty getting the laminate planks to fit together, you should not put them together and take them apart more than three times. This could damage the laminate flooring and mar the effect when you have it completed. 

If you are installing laminate flooring in your kitchen, you should have the cabinets in place beforehand. This is not the case when installing hardwood flooring, but you have to remember that the hardwood is solid wood, whereas laminate flooring is made from engineered wood. It does not have the same level of hardness. This means that you will have to learn how to install laminate flooring around the cabinets. This is also why you need to have a saw to cut the planks when you need smaller sizes and pieces to fit around the cabinets. 

When installing laminate flooring in the laundry room, you should make sure that you have rubber pads underneath the washer and dryer. This is to make sure that these appliances are level so that they won’t damage your flooring. Although most people do not have laminate flooring in the laundry room, there is no reason why you can’t use this room of the house to learn how to install laminate flooring. You can even practice installing hardwood flooring on this small area before you tackle more visible rooms of the house. 

You might be in need of a few tips for installing laminate flooring if you are just learning how to install laminate flooring. If you have to place the laminate flooring around pipes, one tip is to drill a hole in the plank about ¾ to ½ inch larger than the circumference of the pipe. Then cut the plank through the center of the hole and fit the two pieces of laminate flooring together around the pipe and glue them together. When installing laminate flooring, the flooring should extend under the doorframe. If you use a piece of scrap that you have left over, you can use this as a marker for the depth that you need to trim the doorframe.


